[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={77f49320-16ef-11d2-ad51-006097b514dd}
ClassName="D12TEST"
provider=%PHILIPS%
DriverVer=8/13/2001,2.0.0.1278

[Manufacturer]
%MfgName%=Philips

[Philips]
%USB\VID_0471&PID_1625.DeviceDesc%=D12TEST.Dev, USB\VID_0471&PID_1625

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
;DefaultDestDir = 12;that is: $(WINNT)\System32\Drivers
D12TEST.Files.Ext = 10,System32\Drivers
D12TEST.Files.Inf = 10,INF

[SourceDisksNames]
1 = "Install Disk",Disk1,,

[SourceDisksFiles]
D12TEST.sys=1

[D12TEST.Dev]
CopyFiles=D12TEST.Files.Ext
AddReg=D12TEST.AddReg

[D12TEST.Dev.NT]
CopyFiles=D12TEST.Files.Ext
AddReg=D12TEST.AddReg

[D12TEST.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,D12TEST.sys
HKLM,"System\Currentcontrolset\Services\D12TEST\Parameters","MaximumTransferSize",0x10001,65536
HKLM,"System\Currentcontrolset\Services\D12TEST\Parameters","DebugLevel",0x10001,2

[D12TEST.Files.Ext]
D12TEST.sys

[D12TEST.Dev.NT.Services]
Addservice = D12TEST, 0x00000002, D12TEST.AddService

[D12TEST.AddService]
DisplayName    = %D12TEST.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 2                  ; SERVICE_AUTO_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\D12TEST.sys
LoadOrderGroup = Base

[ClassInstall32]
AddReg=D12TESTAddRegClass

[D12TESTADDRegClass]
HKR,,,,%D12TESTClassName%
HKR,,Class,,%D12TESTClassName%
HKR,,EnumPropPages32,,"D12TESTprop.dll,EnumPropPages"
HKR,,Icon,,"127"

;---------------------------------------------------------------;

[Strings]
PHILIPS="Philips Semiconductors"
MfgName="Philips"
USB\VID_0471&PID_1625.DeviceDesc="海信税控器HK_F16G"
D12TEST.SvcDesc="海信税控器HK_F16G"
